{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":55,"n_cols":12,"rows_kept":55,"merged":[[0,0,0,11],[2,8,2,9],[2,10,2,11],[3,8,3,9],[3,10,3,11],[6,0,6,3],[6,7,6,11],[8,0,8,6],[10,0,11,3],[10,7,11,7],[13,0,13,11],[18,11,20,11],[20,7,22,7],[22,11,24,11],[24,7,28,7],[29,7,30,7],[32,11,38,11],[34,7,36,7],[35,3,40,3],[40,11,44,11],[41,3,44,3],[45,3,53,3],[45,7,50,7],[45,11,49,11],[52,7,53,7],[54,0,55,11]]}
["ANNUAL VEHICLE INSPECTION REPORT"]
[{"$nulls":8},"REPORT #",null,null,"FLEET UNIT NUMBER"]
[]
[{"$nulls":8},"DATE"]
[]
["MOTOR CARRIER OPERATOR",{"$nulls":6},"INSPECTOR'S NAME (Print or Type)"]
[]
["ADDRESS"]
[]
["VEHICLE TYPE  (Circle One)",{"$nulls":6},"VEHICLE IDENTIFICATION"]
["Tractor              Trailer                Truck",{"$nulls":8},"LIC. PLATE NO."]
[{"$nulls":9},"VIN"]
[]
["VEHICLE COMPONENTS INSPECTED"]
["OK","Needs Repair","Repaired Date","ITEM","OK","Needs Repair","Repaired Date","ITEM","OK","Needs Repair","Repaired Date","ITEM"]
[{"$nulls":3},"BRAKE SYSTEM",{"$nulls":3},"FUEL SYSTEM",{"$nulls":3},"FRAME"]
[{"$nulls":3},"a. Service Brakes",{"$nulls":3},"a. Visible leak",{"$nulls":3},"a. Frame Members"]
[{"$nulls":3},"b. Parking Brake System",{"$nulls":3},"b. Fuel tank filler cap missing",{"$nulls":3},"b. Wheel Clearance"]
[{"$nulls":3},"c. Brake Drums or Rotors",{"$nulls":3},"c. Fuel tank securely  attached",{"$nulls":3},"c. Adjustable Axle Assemblies (Sliding Subframes)"]
[{"$nulls":3},"d. Brake Hose",{"$nulls":3},"LIGHTING DEVICES"]
[{"$nulls":3},"e. Brake Tubing",{"$nulls":3},"All lighting devices and reflectors required by Section 393 shall be operable."]
[{"$nulls":3},"f. Low Pressure Warning",{"$nulls":7},"TIRES"]
[{"$nulls":3},"g. Tractor Protection Valve",{"$nulls":7},"a. Tires on any steering axle of a power unit."]
[{"$nulls":3},"h. Air Compressor",{"$nulls":3},"SAFE LOADING"]
[{"$nulls":3},"i. Electric Brakes",{"$nulls":3},"a. Part(s) of vehicle or condition of loading such that the spare tire or any part of the load or dunnage can fall onto the roadway."]
[{"$nulls":3},"j. Hydraulic Brakes",{"$nulls":7},"b. All other tires."]
[{"$nulls":3},"k. Vacuum Systems",{"$nulls":7},"WHEELS & RIMS"]
[{"$nulls":3},"COUPLING DEVICES",{"$nulls":7},"a. Lock or Side Ring"]
[{"$nulls":3},"a. Fifth Wheels",{"$nulls":7},"b. Wheels & Rims"]
[{"$nulls":3},"b. Pintle Hooks",{"$nulls":3},"b. Protection against shifting cargo",{"$nulls":3},"c. Fasteners"]
[{"$nulls":3},"c. Drawbar/Towbar Eye",{"$nulls":7},"d. Welds"]
[{"$nulls":3},"d. Drawbar/Towbar Tongue",{"$nulls":3},"STEERING MECHANISM",{"$nulls":3},"WINDSHIELD GLAZING"]
[{"$nulls":3},"e. Safety Devices",{"$nulls":3},"a. Steering Wheel Free Play",{"$nulls":3},"Requirements and exceptions as stated pertaining to any crack, discoloration or vision reducing matter"]
[{"$nulls":3},"f. Saddle-Mounts",{"$nulls":3},"b. Steering Column"]
[{"$nulls":3},"EXHAUST SYSTEM",{"$nulls":3},"c. Front Axle Beam and All Steering Components Other Than Steering Column"]
[{"$nulls":3},"a. Any exhaust system determined to be leaking at a point forward of or directly below the driver/sleeper compartment."]
[]
[{"$nulls":7},"d. Steering Gear Box"]
[{"$nulls":7},"e. Pitman Arm"]
[{"$nulls":7},"f. Power Steering",{"$nulls":3},"WINDSHIELD WIPERS"]
[{"$nulls":7},"g. Ball and Socket Joints",{"$nulls":3},"Any power unit that has an inoperative wiper, or missing or damaged parts that render it ineffective."]
[{"$nulls":3},"b. A bus exhaust system leaking or discharting to the atmosphere in violation of standards (1), (2), (3).",{"$nulls":3},"h. Tie Rods & Drag Links"]
[{"$nulls":7},"i. Nuts"]
[{"$nulls":7},"j. Steering System"]
[{"$nulls":7},"SUSPENSION"]
[{"$nulls":3},"c. No part of the exhaust system of any motor vehicle shall be so located as would be likely to result in burning, charring, or damaging the electrical wiring, the fuel supply, or any combustible part of the motor vehicle.",{"$nulls":3},"a. Any U-bolt(s), spring hanger(s), or other axle positioning part(s) cracked, broken, loose or missing resulting in shifting of an axle from its normal position.",{"$nulls":3},"List any other condition which may prevent safe operation of this vehicle."]
[]
[]
[]
[]
[]
[{"$nulls":7},"b. Spring Assembly"]
[{"$nulls":7},"c. Torque, Radius or Tracking Components."]
[]
["CERTIFICATION:  THIS VEHICLE HAS PASSED ALL THE INSPECTION ITEMS FOR THE ANNUAL VEHICLE INSPECTION REPORT IN ACCORDANCE WITH 49 CFR 396."]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}